*A close up of a logo

Description automatically generated*

*TECHNICAL RIDER (WINTER 2020)*

**Input list…**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CH | Instrument | Preferred Mic | FOH Insert | Position/Stand |
| 1 | Kick Drum In | Beta 91/52A | GATE |  |
| 2 | Kick Drum Out | Audix D6 |  | Short Boom |
| 3 | Snare Top | E904/SM57 |  |  |
| 4 | Snare Bottom | E904/SM57 |  |  |
| 5 | Hi-Hats | SM81 |  | Short Boom |
| 6 | Rack Tom 1 | E904/Beta 98 | GATE |  |
| 7 | Rack Tom 2 | E904/Beta 98 | GATE |  |
| 8 | O/H S.R | SM81 |  | Tall Boom |
| 9 | O/H S.L | SM81 |  | Tall Boom |
| 10 | Ride | SM81 |  | Short Boom |
| 11 | Bass DI USC | House DI Box | COMP 1 | SRC |
| 12 | Bass DI USC | M88/Beta 52 |  | Short Boom USC |
| 13 | Guitar SL | SM57/E906 |  | Short Boom SL |
| 14 | Guitar SR | SM57/E906 |  | Short Boom SR |
| 15 | Vocals (MAIN) | SM58 | COMP 2 | Tall Boom |
| 16 | Vocals SL (BV1) | SM58 | COMP 3 | Tall Boom |
| 17 | Vocals SR (BV2) | SM58 | COMP 4 | Tall Boom |

*See above for the ideal set up for Neptune Valley live. Please use equipment as closely related to the above as possible for the best live performance.*

**Front of House…**

A good quality and well-maintained PA system that will provide even coverage for the entire audience, and that will be able to achieve 115db (A weighted) undistorted signal at mix position.

*A close up of a logo

Description automatically generated*

*TECHNICAL RIDER (WINTER 2020)*

**A screenshot of a computer

Description automatically generated**

If possible, please include a drum riser with dimensions of no less that 8’ x 8’ (2m x 2m is too small). On headline shows, where reasonable space allows, we reserve the right to keep all equipment in-place for the show. When equipment striking is necessary, please ensure that adequate storage space with DIRECT access to stage is provided.

***NO EQUIPMENT TO BE SHARED WITHOUT EXPLICIT AGREEMENT FROM THE TOUR OR PRODUCTION MANAGEMENT. IT IS THE VENUE AND PROMOTERS RESPONSIBILITY TO ENSURE THAT ALL ARTISTS BOOKED TO PLAY BRING THEIR OWN EQUIPMENT.***

**Load-outs…**

Suitable security must be available to facilitate load-outs. This is especially important if required to be done through a crowd. A touring band has a great deal of heavy equipment that is difficult to manoeuvre.

***No liability will be accepted for venue/crowd damage and/or injury caused by loading out, when reasonable assistance/security has not been provided.***

Thank you for your assistance and understanding.

Kind Regards,

NV