Technical Rider

2x Di box line in on stage for laptop – if not phono in to mixing desk

2 power sockets – 1 for laptop, 1 for wireless mic (if possible – otherwise use of house mic)

If possible floor monitoring for backing track and vocals with reverb