Kukushai – Technical Rider

Acoustical piano or keyboard KORG SV1:

* 2x jack for the effects output( effects are running parallel with dry signal)
* 2x jack out for dry keyboard or acoustical piano amplified with 2 microphones for the stereo image + additional bass microphone for the low end

Vocal:

* Voicelive touch 2 effect, 2x jack out
* 2xjack for the synth

Drums:

* jazz/fusion kit with kick, floor, tom, snare, hihat, various cymbals
* microphones 2xOH, kick, snare ( or the whole kit)

Position from L to R( audience perspective): drums, vocal, piano. Each member needs a monitor.\*