**SicNis – Technical requirements 2018**

**Acoustic Band**

**Unless otherwise agreed, an adequate PA and sober, competent sound engineer must be supplied to suit the venue. The band will require on stage monitoring with a minimum of 2 wedges.**

|  |  |
| --- | --- |
| **Lead Vocal** | 1x Wireless Mic or SM58  1x Mic Stand |
| **2x Backing Vocals** | 2x SM58  2x Mic Stand |
| **Acoustic Guitar** | 1x DI |