|  |  |
| --- | --- |
|  | SonicTribe d.o.o.  Podmilščakova 16,  1000 Ljubljana, Slovenija  st@sonictribe.net |

**MRFY**

TECHNICAL RIDER

The band’s team

**BAND MEMBERS**

**Gregor Strasbergar** | main vocal, guitar

**Tomaž Zupančič** | kitara, back vocal

**Lenart Merlin** | bass guitar, back vocal

**Rok Klobučar** | drums

**CONTACT**

**Gregor Strasbergar** | 070 831 705

**Žiga Blazinšek** | 040 878-380

**AUDIO ENGINEER**

**Gregor Bajc** | 051 606 820

**ADDITIONAL INFO**

**mrfy.official@**gmail.com  
**facebook**.com/pg/MRFYnm

**instagram**.com/mrfy\_band/

**About:** [www.sonictribe.net/mrfy](http://www.sonictribe.net/mrfy)

Requests

**SOUND CHECK**

* at least 15 minutes for preparation of stage needed and
* at least 45 minutes for soundcheck needed

**2x Vocal**Front stage, center and right

**2x Guitar**

Lead Guitar 2 amplifiers (combo Crate Vintage tube 30 2x12 + mini Vox ) + pedalboard

Vocalist – Rhythm guitar (DV Mark Galileo amplifier and DV Mark 2x12 box) + pedalboard + DI box for acoustic

**Bass Guitar:**

Markbass amp, box Markbass 4x10

**Drums:**

* 1x Snare,
* 1x Kick
* 1x Hanging tom,
* 1x floor tom,
* 1x crash
* 1x ride
* hihat

**STAGE PLOT**

|  |
| --- |
|  |

**IMPORTANT**

The doors of the club should be closed until the soundcheck ends.

Front of the house requirements

**A MINIMUM REQUIREMENT**

An analog/digital mixer with at least 16 inputs/outputs and 2 send/return FX channels (4 if available for optimum sound performance)

**INPUT LIST**

(May vary depending on the venue, please ask the SE for opinion at venue, also the choice of microphones must be discussed, based on availability)

1. Kick / Insert: Gate>Compressor
2. Snare Top / Insert: Compressor
3. Snare Bottom / Insert: Gate>Compressor (if possible)
4. Floor Tom / Insert: Gate>Compressor
5. Hi Hat
6. Ride
7. OH L (if place needs overheads)
8. OH R (as before mentioned, if place needs them)
9. Bass DI (DI BOX) / Insert: Compressor
10. Bass Mic
11. Guitar Left (solo guitar)
12. Guitar Right (singer guitarist)
13. Vocal Front Left (lead guitarist)
14. Vocal Front Center (Main Vocal,Rythm guitarist) Insert: >Compressor
15. Vocal Front Right (bassist)

**FX**

2 FX are a minimum for the band perform, 4 are optimum if available.:

* Reverb #1: Drum Room (1,2 sec, Wide, If available)
* Reverb #2: Hall Reverb (3-4 sec) (Minimum!)
* Reverb #3: Plate Reverb (1 sec) (If available)
* TAP Delay #4: (MINIMUM!)

Each of these sends should have stereo returns tracks, on which the sound engineer should have the possibility of signal processing.

Hospitality rider

* Warm meal
* 2 litres of wine
* 2 liters of sparkling water
* Jameson+Sprite or Gin+Tonic or Vodka+RedBull
* 1 litre of orange juice
* Bottled water