TECHNICAL RIDER FOR QUEEN MARILYN 1

1. Microphone Cordless Shure BLX2/PG58-T11 Wireless Handheld Microphone Transmitter

Specifications

Form Factor: Handheld

Wireless Frequency: 863MHz - 865MHz

Operating Range (Up To): 100 m (Under Typical Conditions)

Transmitter Housings: Moulded ABS

Audio Mute: No

Detachable Antennas: No

Switchable RF Power: No

Batteries: AA

Battery Status: Multi-Colour LED

Frequency Diversity: No

Functionality: Transmitter

High Density Mode: No

Weight: 340 g

Transmitter Weight: 218 g

Dimensions:

Height: 224 mm

Width: 53 mm

Depth: 53 mm

1. With ear monitors (provided by the artist)

JTS 4 Channel Monitoring Mixer

Power Supply: 12-18Vdc, 600mA
Inputs: 4 x 1/4" Jack/XLR Combo Sockets
Aux Input: 2 x 1/4" Jacks
Output: 1/4" Jack
Dimensions: 205 x 212 x 43.5mm
Weight: 1.4Kg

Ear Monitors JTS IE-1 High Defination Dynadriver Earphone

Response: 20Hz-20kHz
Sensitivity: 114db
Impedance: 16 Ohms
Cable Length: 1480mm
Weight: 6g

JTS In-Ear Monitoring System Bodypack Receiver

Carrier Frequency: 863-865MHz

1. Stage speakers provided by Venue
2. Mixing desk provided by venue

|  |  |
| --- | --- |
| Product model number | DX360CF |
| EAN | 5011139072191 |

1. 2 Stage fans (provided by artist) Freestanding, 360 fan

|  |  |
| --- | --- |
| Depth (mm) | 204 |
| Height (mm) | 340 |
| Weight (kg) | 1.9 |
| Width (mm) | 275 |

|  |  |
| --- | --- |
| Cable Exit Point | Back |
| Cable Length (m) | 1.8 |
| Carry Handles | Yes |
| Electric supply | 230-240V ~ |

|  |  |
| --- | --- |
| Oscillating function | 360 |

|  |  |
| --- | --- |
| Suitable for which room/s | Any room. |

STAGE LIGHT: Provided by venue alternatively Artist will have on standby

1. 1 COB Plano Compact LED Par Can 36 Watt RGB

Mains Input: 100-240Vac, 50/60Hz
Power Consumption: 40w
LED's: 36w COB
Beam Angle: 100 Degrees (Without Lens)
15 Degrees (With Lens)

Dimensions: 202 x 120 x 224mm

Weight: 2Kg

1. 1 Slim Hex Par RGBAWUV 12 x 10 Watt LEDs

Power Supply: 230Vac, 50Hz
Power Consumption: 70w
LED: 12 x 10w RGBWA & UV
Beam Angle: 25 Degrees
DMX Channels: 6 or 10
Dimensions: 270 x 252 x 90mm
Weight: 3Kg

1. 2 Light Stands

Max Height: 3.4m
Folded Length: 1.4m
T-Bar: 1.2m
Max Load: 30kg