*İSTANBUL KAİNAT RADYOSU (İSTANBUL UNIVERSE RADIO)*

 **INPUT CHANNEL LİST**

|  |  |  |  |
| --- | --- | --- | --- |
| **CH** | **ENSTRUMAN** | **MIC/DI** | **STAND** |
| 1 | Cajon (front) | SHURE SM 57 | KISA |
| 2 | Cajon (back) | SHURE BETA 91 | BOOM |
| 3 | UDU DRUM | SHURE SM 57 | BOOM |
| 4 |  FRAME DRUM | SHURE SM 57 | BOOM |
| 5 |  ROLAND HDP 20 (electronic) | TS Jack | DI-BOX |
| 6 |  ROLAND HDP 20 (electronic) | TS Jack | DI-BOX |
| 7 | OH R | CONDENSER | BOOM |
| 8 | OH L | CONDENSER | BOOM |
| 9 | BASS | BASS AMP or DI-BOX + TS JACK |
| 10 | BASS (fretless) | BASS AMP or DI-BOX + TS JACK |
| 11 | TANBUR (BOWED LONG NECK LUTE) | \*E 614 CONDENSER | BOOM |
| 12 | TROMPED | \*\*SD-SYSTEMS LCM77 |
| 13 | KEYBOARD | DI-BOX + TS JACK |
| 14 | KEYBOARD | DI-BOX + TS JACK |
| 15 | LEAD VOX  | SHURE SM 58 | BOOM |
| 16 | LEAD VOX (bass) | SHURE SM 58 | BOOM |
| 17 | BACK VOX (Lute) | SHURE SM 58 | BOOM |
| 18 | BACK VOX (key) | SHURE SM 58 | BOOM |
| 19 | BACK VOX (tr) | SHURE SM 58 | BOOM |

**\*If this E-614 mic. cannot be found, replace AKG C-411**

**\*\* Or a replacement microphone**

**AUX (MONITOR)) CHANNEL LIST**

|  |  |  |
| --- | --- | --- |
|  | **AUX** | **MONITOR**  |
| **1/2** | LEAD VOX | **IEM+ Floor monitor** |
| **3/4** | BASS, VOX | **IEM+ Floor monitor** |
| **5** | BACK VOX(TANBUR (LUTE)  |  **IEM** |
| **6** | **BACK VOX**(TROMPED) |  **IEM** |
|  **7** |  BACK VOX (KEYBOARD) |  **Floor monitor** |
|  **8** |  BACK VOX.  (PERCUSSION) |  **IEM**  |
| **9/10** | SIDE FILL | 2 PEACES , 3 WAY SPEAKERS  |

 **BACKLINE EQUIPMENT LIST**

|  |  |
| --- | --- |
|  **Piece** | EQUIPMENT  |
| 1 | HI-HAT STAND |
| 5 | SYMBAL STAND |
| 1  | DRUM CARPET  |
| 1 | KEYBOARD (ROLAND FA-80 or FP-80 |
| 1 | Senheiser E 614 CONDENSER MIC |
| 1 | SD-SYSTEMS LCM77 |
|  1 | GK BASS AMPLIFIER  |
| 3 |  ELECTRICITY (Key, bass, perc) |
| 2 |  BASS STAND |
| 1 |  DOUBLE KEYBOARD STAND |
| 1  |  LUTE STAND (Classical guitar stand correct) |
| 5 |  TS JACK |
| 11 |  BOOM STAND |
| 1  |  SHORT BOOM STAND |