- mixer with at least 12 channels (12 mono or 4 stereo + 4 mono) + 2 AUX post fader send, 4 bus (Midas, Mackie, Allen & Heath or similar). All my connections are 1/4" TSR Jack
- good stereo monitors
- TABLE SPACE TO SETUP NO LESS THAN 1.5m x 1m AND OF GOOD HEIGHT (1.1 m or so)
- 9 power plugs 

I need 1 hour for setup and soundcheck.